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IDENTIFICATION LABEL


LOCATION
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X
See the Attached Photograph or Sketch






Back of Radio






Back of Radio under Belt Clip


TYPE





X
The label is a paper polyester firm laminate with a pressure 






sensitive adhesive backing. The adhesive is a permanent type 





acrylic with a minimum peel strength of 40 oz/inches.






The label is laser etched into the Urethane paint, exposing the






Nickel plating on the Zamak casting substrate. Since no adhesive






Is required, the label is permanent and tamper-proof. 






(**-NOTE- The label attached below is a paper polyester film 






laminate, as described above. This is just for sample purposes, as 






the actual label is laser etched into the casting)
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See the Attached Photograph
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Label Attached Below






See Attached Drawing







GENERAL INFORMATION
l.
Production Plans -- Pursuant 2.981 ( c )



Quantity production is planned

ll.
Application References -- Pursuant 2.1061

EIA/TIA-603 Land Mobile FM or PM Communications Equipment Measurement and Performance Standards



Code of Federal Regulations Title 47, Part 2, Sec. 2.983-2.999 and Part 90, Sec.90.210         

lll.
Data Submittal Procedure:



Data is supplied in accordance with Part 2, Sub-part J of the Commissions’ Rules.

The intended use of this transceiver includes applications covered in the Code of Federal Regulations Title 47, Parts 22, 74, and 90.








